**Technical Bid Annexure-II**

 **WORK SPECIFICATION OF INTERIOR DECORATION OF THE BOARD ROOM ON 2 ND FLOOR OF HEAD OFFICE**

 TAMLUK-GHATAL CENTRAL CO-OPERATIVE BANK LTD. TAMLUK,PURBA MEDINIPUR

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **SL. NO** | **WORK-TYPE** | **WORK- SPECIFICATION** | **ITEAM DETAILS & APPROVED BRANDS/ MANUFACTURERS** | **BIDDER COMMENTS** |
|  |  |  | (A)PROVIDING & FIXING OF FALSE |  |
| **1.** | **FALSE CEILING** | POP/GYPSUM | CEILING WITH EXPOSED G.I. GRIDE |
|  |  | BASED **ROYAL** | SUSPENSION SYSTEM (E-GRID U- |
|  |  | **AESTHETIC** | 1520 OR EQUIVALENT LOAD |
|  |  | **LOOKS** FALSE | CARRYING CAPASITY WITH3600 |
|  |  | CEILING WITH | MM LONG,CROSS TEE |
|  |  | DESIGN | 1200MM/600MM LONG & WALL |
|  |  |  | ANGLE.THE WALL ANGLE SHALL |
|  |  |  | BE FIXED BY FASTENERS. |
|  |  |  | (B)ACCOUSTIC FALSE CEILING |  |
|  |  |  | MADE BY GYPSUM BOARD |
|  |  |  | (C) GROUP DESIGN ON SIDE DROP |  |
| **BRAND**- India Gypsum, Lafarge Gypsum  |  |
| **2.** | **ELECTRIFICATION** | TOTAL | (A)ELECTRIFICATION WITH |  |
|  |  | CONCEALED | CONCEAL WIRING BY 0.5 SQ |
|  |  | WIRING WITH | MM,0.75 SQ MM, 1.5 SQ MM, 2.5 |
|  |  | LIGHTS & FANS | SQ.MM ,4.0 SQ MM WIRE |
|  |  |  | **BRAND - FINOLEX / POLYCAB** |
|  |  |  | (B) SWITCHES,BOARD,PLATE  |  |
|  |  |  | **BRAND**- ANCHOR ROMA/HAVELLS CRABTREE |
|  |  |  | (C) MCB & DB BOX BRAND- L& T /LEGARD |  |
|  |  |  | (D) 20 WATT 4K LED PANEL LIGHTS (20 PCS)  |  |
|  |  |  | BRAND- PHILIPS/PANASONIC/CROMPTON |
|  |  |  | (E) WALLFAN (12”) –5 Pcs |  |
|  |  |  | BRAND -**C**ROMPTON /HAVELLS |
|  |  |  | (F)8WATT - COB SPOT LIGHTS (20 PCS PCS |  |
|  |  |  | BRAND - PHILIPS/PANASONIC/CROMPTON |
|  |  |  | (G)PROFILE LIGHTS |  |
|  |  |  | (F) MODERN BRACKET LIGHTS (15PCS) |  |
|  |  |  | BRAND - PHILIPS/PANASONIC/CROMPTON |
|  |  |  | (G) CHANGE OVER SWITCH BRAND- HPL / HAVELLS  |  |
| 3 | GLASS |  DOOR, WINDOW  | SAINT GOBIN /MODIFLOAT |  |
|  | Aluminum Sections  |  WINDOW PANEL etc. | LYCO |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **4** | **PUTTY & COLOUR** | CEILING | ASIAN PAINTS/ICI DULUX PUTTY & ROYAL OIL BASED PRIMER |  |
|  |  |  | ASIAN PAINTS ROYAL SHYNE/ICI DULUX VELVET TOUCH COLOUR |  |
| **5** | **PLYWOOD****,LAMINATES & HARDWARE FITTINGS** | FULLCEILINGLENGTH WALL PANELLING WITH BACK STRUCTURE BY 19 MMPLYWOOD ON TWO SIDES OF WALL | 19 MM THICK ISI CERTIFIED PLYWOOD |  |
| **4.0 MM GREEN/CENTURY VENEER PASTING OVER PLYWOOD** |  |
| **PREMIUM GRADE PU POLISH****BRAND-ASIAN PAINTS PU EMPORIO** |  |
| **12 MM PLYWOOD WALL PANELLING WITH 1.5 MM THICK STEEL****STRUCTURE** |
| **1.5 MM THICK STEEL STRUCTURE** |  |
| 19 MM PLYWOODMAKE TABLE | HARDWARE FITTINGS WITH FITTING & FIXING BRAND-GREEN PLY/CENTURY |  |
| **VENEER PASTING** |
|  **PU POLISH** | **BRAND-ASIAN PAINTS PU EMPORIO** |  |
| **6** | **LOUVERS** | LOUVERS DIGITAL PLANKS | LOUVERS DIGITAL PLANKS USEDBRAND-HUTCH |  |
| **7** | **T-PROFILE** | T-PROFILE WALL | GOLD T-PROFILE ON WALLBRAND-DELICA |  |
| **9** | **Door Lock / Door Handles** | DOOR | BRAND- HETTICH |  |
| **10** | **DOOR CLOSURE** |  | BRAND -Godrej / Archi  |  |
| **11** | **PVC MOULDING BIT** | PVC MOULDING BIT WITH NAIL FREE JOINING | PVC MOULDING BIT WITH NAIL FREE JOINING |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **12** | **WOODEN FLOORING** | WOODEN FLOORING | WOODEN 10.0 MM THICK PVC INTERLOCKING FLOORING .BRAND-MIKASA /ARMSTRONG |  |
| **13** | **ROMAN BLINDS** |  | ROMAN BLINDS AS REQUIRED |  |
| **14** | **LAN CONNECTION** | LAN CONNECTION ON TABLE | LAN CONNECTION ON TABLECAT 6 BRAND-DLINK |  |
| **15** | **SOUND SYSTEM** | **JBL** SOUND SYSTEM WITH SPEAKERS | **WATT CEILING SPEAKERS ( 6****PCS)** |  |
| JBL GM -601 LM **GOOSE NECK MICROPHONE (30 PCS)** |  |
| JBL AMPLIFIER (1 PCS) |  |

 **Signature of the Bidder with seal**