ANNEXURE-A

INTERIOR DECORATION & FURNISHG WORK, ELECTRICAL,SOUND SYSTEM OF THE MEETING HALL ON 2ND FLOOR OF TAMLUK-GHATAL CENTRAL CO –OPERATIVE BANK LTD, TAMLUK, PURBA MEDINIPUR

(AREA-1890 SQ.FT)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **SL. NO** | **WORK- TYPE** | **WORK- SPECIFICATION** | **ITEAM DETAILS & APPROVED BRANDS /MANUFACTURERS** | **SAMPLE PICTURE** |
| **1.** | **FALSE CEILING** | POP/GYPSUM BASED **ROYAL AESTHETIC LOOKS** FALSE CEILING WITH DESIGN **& ROYAL DOME** | (A)PROVIDING & FIXING OF FALSE CEILING WITH EXPOSEDG.I. GRIDE SUSPENSION SYSTEM (E-GRID U-1520 OR EQUIVALENT LOAD CARRYING CAPASITY WITH3600 MM LONG,CROSS TEE 1200MM/600MM LONG & WALL ANGLE.THE WALL ANGLE SHALLBE FIXED BY FASTENERS. |  |
| (B)ACCOUSTIC FALSE CEILING MADE BY 30”\* 36**”** POPBOARD/GYPSUM |
| (C) MOUILDING BIT (4” THICK )ON THE FACE OF SIDE TRAY |
| (D) AESTHETIC LOOKS DOME (4’ RADIUS) |
| **BRAND**-India Gypsum, Lafarge Gypsum  |
| **2.** | **ELECTRIFIC ATION** | TOTAL CONCEALED WIRING WITH LIGHTS & FAN | (A)ELECTRIFICATIONWITH CONCEAL WIRING BY 0.5 SQ MM,0.75 SQ MM, 1.5 SQ MM,2.5 SQ.MM ,4.0 SQ MM FINOLEXWIRE**BRAND - FINOLEX / POLYCAB** | **Bracket Light** |
| (B) SWITCHES,BOARD,PLATE  |
| **BRAND-**ANCHORROMA/ HAVELLS /CRABTREE |
| (C) 20 WATT 4K LED PANEL LIGHTS (70 PCS)  |
| **BRAND- PHILIPS/PANASONIC/CROMPTON** |
| (D)8WATT - COB SPOT LIGHTS (50 PCS ) |
| BRAND - **PHILIPS/PANASONIC/CROMPTON** |
| ROPE LIGHTS WITH ADAPTER |
| (E) **VINTAGE** BRACKET LIGHTS (15PCS) **BRAND - PHILIPS/PANASONIC/CROMPTON** |
| (F) MCB & DB BOX **BRAND- L& T /LEGARD** |  |
| (G) WALL FAN (12”) –25 Pcs**BRAND-CROMPTON/HAVELLS** |
| **3** | **PUTTY & COLOUR** | WALL & CEILING | ASIAN PAINTS /ICI DULUX PUTTY & ROYAL OIL BASED PRIMER |  |
| ASIAN PAINTS ROYAL SHYNE/ICI DULUX VELVET TOUCH COLOUR |  |
| **4** | **POP BIT/PILLAR****/HEAD** | ORNAMENTATION | POP MAKE MOULDING BIT (71MM THICK) WITH FITTING & FIXING ON WALL |  |
| POP **WALL PILLAR** (ROUND) DIMENSION- H2438 MMX202MM WITH FITTING &FIXING |
| **DECORATIVE HEAD** OVER PILLAR (SIZE-H308MMX W495MMX210MM) WITHFITTING & FIXING |
| POP STRAIGHT PILLAR (SIZE- H2362 MMX W240MM) |
| **5** | **PLYWOOD & VENEER** | WALL PANELLING WITH BACK STRUCTURE & ROYAL DESIGN WITH VENEERPASTING | 19 MM THICK  |  |
| 4.0 MM MAKE VENEER**BRAND - GREENPLY****/CENTURY PLYWOOD** |
| MAIN PILLAR FULL HEIGHT PANELLING WITH ROYAL WORK & VENEER PASTING |
| 12 MM TOUGHEN GLASS DOORS |
| DIAS &PODIUM |
| ENTRY GATE &GLASS DOORS | **BRAND-SAINT GOBIN /MODIFLOAT** |
| **6** | **WOODEN WORK** | WOOD MAKE SKIRTING & BIT | SAGOON WOOD MAKESKIRTING MOULDING BIT (6’’) |   |
| SAGOON WOOD MAKE MOULDING BIT (4”) OVERPLYWOOD PANELLING |
| SAGOON 1” BIT ON VENEER |
| BATALI DESIGN WORK |
| **7** | **PU & DUCO POLISH** | PREMIUM QUALITY PU MATT FINISH | **PU SEMI-MATT FINISH** PREMIUM QUALITY POLISH ON VENEER & **DUCO** POLISH ON PARIS BITBRAND - **ASIAN PAINTS PU EMPORIO** **ASIAN PAINTS DUCO POLISH WITH GLITTERING EFFECT.** |  |
| **8** | **WOODEN PVC FLOORING** | WOODEN FLOORING | WOODEN 10 MM THICK PVC INTERLOCKING FLOORINGBRAND-MIKASA /ARMSTRONG |  |
| **9** | **CURTAIN** |  | **ROYAL** LOOKS DOUBLE HEAVY PREMIUM CURTAIN |  |
| **10** | **LAN CONNECTI****ON** | LAN CONNECTION ON TABLE | LAN CONNECTION ON TABLECAT 6 **BRAND -DLINK** |  |
| **11** | **PELMET** |  | PLYWOOD & VENEER PASTING PELMET WITH WOODEN BATALIWORK DESIGN & POLISH |  |
| **12** | **SOUND SYSTEM** | **JBL** SOUND SYSTEM WITH SPEAKERS | 30 WATT CEILING SPEAKERS (12PCS) |  |
| FRONT BOX 12 ‘’ (2 PCS) |  |
| AKG MINI 2 DUAL WIRELESSMICROPHONE (2PAIR) |  |
| JBL GM -601 LM GOOSE NECKMICROPHONE (5 PCS) |  |
| JBL AMPLIFIER (2 PCS) |  |
| **13** | **WALLPAPE R** | PREMIUM BELGIUM WALLPAPER | ROYAL LOOKS PREMIUM QUALITY BELGIUM MADE WALLPAPER AS REQUIRED |  |
| **14** | **WINDOW CHANEL** | COATED ALUMINIUM SLIDING WINDOWS WITH ONE VISION5MM GLASS | COATED ALUMINIUM SLIDING WINDOWS (12 PCS) WITH GLASS (ONE VISION)BRAND- **LYCO** |  |